|  |
| --- |
| Operator Name:  Date: |
| **Demonstrate the following procedures whilst disconnected from the power**   |  |  | | --- | --- | | Raise and lower wheeled stand |  | | Inspect top door for tracking |  | | Inspect bottom door for cleanliness |  | | Check integrity of blade |  | | Check blade tension |  | | Set guard the correct distance from the top of the workpiece. |  |   **Demonstrate the following procedures whilst connected to power**   |  |  | | --- | --- | | Listen for sound of bent/broken teeth |  | | Make straight cut |  | | Make curved cut on appropriate bandsaw |  |   **Understand the following things**   |  |  | | --- | --- | | How to report faults (users should not fix problems themselves) |  | | Meaning of no lone working rule |  | | Blade needs to be at full speed before introduction of material |  | | How to select mitre or rip guard |  | | Which PPE is required or recommended (goggles required, breathing and hearing protection recommended; gloves not to be worn) |  | | Hands should be 15cm from the blade during operation |  | | Push sticks are required when closer than 15cm |  | | Use of vee block when cutting round items |  | | Need to disconnect power whilst inspecting the blade |  | | Users must not enter yellow box areas when another user is using a power tool in that area |  | | Users must inform other hackspace users if they are cutting anything with higher than average respiratory risks |  | | Dust extraction must be used where available |  | | Machine is used for wood only or some plastics |  | | User is responsible for cleaning up |  | |

When competence has been achieved, tick the appropriate requirement.